
 CH Pro Throttle Configuration and Hints for use with Fighter Duel 1 and
 NetDuel. - 6 November, 1996

 First off, the Pro Throttle DOES work with Fighter Duel.  The confusion
 on whether it works or not comes from the different handling of certain
 keystrokes in Fighter Duel, and how the Pro Throttle sends them through
 the keyboard interface (which is *very* close to how a keyboard sends
 but *not* identical in all cases).

 Hint No. 1: For keys which are toggles, set them as "Macros" in the Pro
 Throttle.  This will cause them to be sent once each time you hit them
 instead of repeatedly.  An example of this is the Boost key (B).

 Hint No. 2: For keys which are only active when pressed, set them as
 "Sent until released" in the Pro Throttle.  This will cause the throttle
 to continually send them as pressed while you are pressing the button. 
 An example of this is the Label (L) key in NetDuel.

 Two example Pro Throttle configuration files are included. Our own, FD1.PTC
 and FD2.PTC which is configuration file supplied by an avid Fighter Dueler.
 FD1.PTC has the following mappings:

 Button 4    - Left brake
 Button 3    - Both brakes on/off
 Button 2    - Right brake
 Button 1    - Boost

 Hat 4 Up    - Turbo                      Hat 2 Up    - Chatter (ND)
 Hat 4 Down  - Launch                     Hat 2 Down  - Toggle IAS/TAS
 Hat 4 Left  - Save PCX                   Hat 2 Left  - Toggle Hud
 Hat 4 Right - Trim reset                 Hat 2 Right - Labels (ND)

 Hat 1 Up    - Chase view (F1)            Hat 3 Up    - Flaps up
 Hat 1 Down  - South view (F4)            Hat 3 Down  - Flaps down
 Hat 1 Left  - Down from 4,000 ft (F11)   Hat 3 Left  - Gear control
 Hat 1 Right - Down from 30,000 ft (F12)  Hat 3 Right - Hook control

 Button 1 is on the rear of the unit, buttons 2-4 are on the front going
 from right to left.

 Hat 4 is on the front of the unit, hats 1-3 are on the rear of the unit
 with 1 in the middle position, 2 on top, 3 on bottom. Up/Down presses
 are relative to reality. Hat 4-Left press pushes it towards the buttons
 and Right pushes it away.  For hats 1-3 Left pushes go in the direction
 of Button 1 and Right pushes them away.

 Sorry if this is a little confusing, but this IS how they are identifies
 by the CH Pro Throttle setup utility.  Unfortunately there is no diagram
 included with the Pro Throttle (at least with my unit) so it's not very
 clear.

 
